ESSVE

Press release

December 2012

Façade plug GXL

One façade plug is enough!

Now there’s no need to spend time thinking about which façade plug to use for fastening in walls of different materials. Façade plug GXL from ESSVE is a new universal plug for fastening in all kinds of materials such as concrete, massive brick, calcareous sandstone, lightweight concrete, hollow core slab, and hollow brick. That makes the GXL an ideal screw for fixing frames, beams, consoles and kitchen carpentry in both hard and porous material, indoors as well as out.

Just like other façade plugs from ESSVE, the new GXL is available in a set with an attached screw as well as individually in bulk. GXL is available in the corrosion classes C1 and C3, i.e. electro-zinc plated and hot-dip galvanized respectively. GXL is also available with a countersunk head for use in wood and a HEX-head for use in metal.

Fasten façade plug GXL in all these wall materials:

▪ Concrete

▪ Massive brick

▪ Calcareous sand rock

▪ Lightweight concrete

▪ Hollow core slab

▪ Hollow brick

Façade GXL gets it done for these fixing jobs:

▪ Façade fixing

▪ Door frames

▪ Windows

▪ Kitchen interiors

▪ Wardrobes

▪ Hand rails

▪ Doorways

▪ Wooden- and metal constructions

▪ Consoles

▪ Rails

▪ Cable ladders

▪ Angles

**For further information:**

**Mattias Sebell**, Marketing Manager ESSVE,

+46 70 623 28 78, [mattias.sebell@essve.se](mailto:mattias.sebell@essve.se)